**XYTable[] array generator**

**Intro**

This Arduino sketch will create a lookup table for LED projects instead of writing and using mapping code. It uses LEDMatrix definitions (ex: HORIZONTAL\_ZIGZAG\_MATRIX) to define the LED mapping.

The LED mapping apps I have found all have shortcoming on the size or layout of the matrix. Especially for blocks or cells within the matrix like the popular 8x8 blocks. This sketch includes:

Up to 32k LEDs

Small to very large matrices – laid out in any direction with or w/o zigzag

Matrix can be made of blocks (cells) of any size that of any size– laid out in any direction with or w/o zigzag in the block and block layout within the matrix.

Produces a report on the Serial Terminal of the specified configuration and the resulting mapping array.

Simple cut and paste into your header file.

Arduino code in small single purpose functions that are easy to modify

LEDMatrix reference:

<https://jorgen-vikinggod.github.io/LEDMatrix> has an excellent tutorial on mapping definitions.

**OUTPUT:** will be on the serial terminal so you can review the results and make changes.

**TO SAVE:** copy and paste the terminal output array to a file.

**Parameter List Guide**

**================= for width and height ==========================**

Do you have an LED array to start with or an IRREGULAR layout? You can #include it in step 1.

If you have an irregular array, you should 1st create the array with missing LEDs here:

FastLED XY Map Generator: *https:macetech.github.io/FastLED-XY-Map-Generator*

NOTE: make the array simple, left to right and top to bottom, no zigzag.

We will make all these changes here.

**WHEN DESIGNING BLOCKS IN A MATRIX, COMBINATIONS CAN GIVE SURPRISING RESULTS.**

**IF THE RESULT IS NOT WHAT YOU EXPECTS, REVIEW EACH STEP'S SETTINGS AGAIN!**

**STEPS**

1. array name must be*: "const uint16\_t PROGMEM XYTable[][x] = {}"* or:

*"const uint16\_t XYTable[][x] = {}"* The [x] length is required.

PROGMEM is optional. Set PROG\_MEM below as true or false to match

#*define HAVE\_ARRAY false*

*#if HAVE\_ARRAY*

*#include "XYTable\_LookUp.h"* edit your file name here

*#endif*

1. Set the overall Panel size in number of LEDs.

What direction does the FIRST row go?

What direction does the FIRST column go?

LEDMatrix uses a NEGATIVE value for reserved (right to left) and (bottom to top).

| Parameter | Description |

| ------------ |-----------------------------------------------|

| MATRIX\_WIDTH | width of matrix (negative for reverse order) |

| MATRIX\_HEIGHT| height of matrix (negative for reverse order)|

*#define MATRIX\_WIDTH 32 //use negative value for reversed (right to left)*

*#define MATRIX\_HEIGHT 32 //use negative value for reversed (bottom to top)*

1. How are the LEDs in the total matrix organized? (Regardless of and blocks or cells making up the matrix).

**>>>>> If using BLOCKs/cell to make up your matrix, this is n/a. See steps 6 and 7**

*MatrixType\_t matrix\_type = HORIZONTAL\_MATRIX;*

Options: HORIZONTAL\_MATRIX, VERTICAL\_MATRIX, HORIZONTAL\_ZIGZAG\_MATRIX, VERTICAL\_ZIGZAG\_MATRIX

**================= BLOCKS options =================**

1. LEDs make a BLOCK (cell), BLOCKS make up a MATRIX (panel). if you have one long LED string in your display set HAS\_BLOCK false and ignore these BLOCK values

*#define HAS\_BLOCKS true*  Is this matrix made up of block/cells of LEDs?

*#define MATRIX\_TILE\_WIDTH 8* width of each matrix BLOCK/CELL (not total display)

*#define MATRIX\_TILE\_HEIGHT 8* height of each matrix BLOCK/CELL

*#define MATRIX\_TILE\_H 4* the number of tiles arranged horizontally

*#define MATRIX\_TILE\_V 4* the number of tiles arranged vertically

1. How are the LEDs organized inside the block/cell?

*BlockType\_t blockOrg = HORIZONTAL\_BLOCKS;*

Options: HORIZONTAL\_BLOCKS, VERTICAL\_BLOCKS, HORIZONTAL\_ZIGZAG\_BLOCKS, VERTICAL\_ZIGZAG\_BLOCKS

1. How are the block/cells organized in the matrix?

*BlockType\_t blocksInMatrix = HORIZONTAL\_BLOCKS;*

Options: HORIZONTAL\_BLOCKS, VERTICAL\_BLOCKS, HORIZONTAL\_ZIGZAG\_BLOCKS, VERTICAL\_ZIGZAG\_BLOCKS

1. NEW OPTION NOT AVAILABLE IN LEDMatrix ONLY IF USING THIS TABLE LOOKUP METHOD

These 2 flip the order of the tiles/BLOCKS in the matrix

The LED order inside the blocks stay the same

To flip everything in the matrix panel including the LEDs inside the blocks see step 3.

| Parameter | Description |

| ------------ |-----------------------------------------------|

| H\_blockDir | horizontal direction of led flow in the tile |

| V\_blockDir | vertical direction of led flow in the tile |

*MatrixOrder\_horizDir H\_blockDir = LEFT\_2\_RIGHT;* Options: LEFT\_2\_RIGHT, RIGHT\_2\_LEFT

*MatrixOrder\_vertDir V\_blockDir = TOP\_DOWN;* Options: TOP\_DOWN, BOTTOM\_UP

1. DEBUGGING: Add h and v hash marks between blocks for easier viewing you can delete in an editor after copying.

*#define TABLE\_DIVIDERS true* Options: true, false

**================= End BLOCKS =================**

1. DONE - compile and run